## ***EasyClean free UnderSink:* a miracle of space**

# This Grease separator from KESSEL is the fitting solution in space limited places

In food trucks, takeaways, or small restaurants – where only small volumes of wastewater are produced and the space is limited, the *EasyClean free UnderSink* from KESSEL allows for an easy and efficient collection of fats, oils and greases. Optimised for free-standing set-ups in frost-protected rooms, its low weight (5 kg) and compact size (33 l) makes this separator ideal for the wastewater discharge from a sink. By TÜV, it has been tested and approved on the test bench with efficient 0.7 l/s.

**EasyClean = Easy-going**

The *EasyClean free UnderSink* is manufactured from permanently resistant polymer (PP). That makes it 100 % corrosion-free and resistant to wastewater containing aggressive ingredients such as fatty acids. Using this material ensures the separator tank – equipped with an integrated sludge trap (12 l) – is not only durable, but waterproof and odour-tight. A cover with all-round seal and clip closures simplifies cleaning and maintenance measures. To aid installation and removal, the separator has a quick-release, 360° rotatable and vertically adjustable swivel connection to the pipe. Therefore, no tools are needed for installation, cleaning, or remove of the separator. In addition, the narrow tank allows for easy transportation through narrow entranceways.

If the installation of large central grease separators is not possible, the KESSEL *EasyClean free UnderSink* offers a solution where space is limited. This option combines easy, tool-free installation, cleaning performance and energy efficiency for kitchen with small quantities of wastewater – or to keep it simple: a little miracle of space.

**This is KESSEL**

Since 1963, KESSEL has stood like no other company for quality, innovation, safety and service in the field of draining technology. As a premium international provider and industry pacesetter, we continuously strive to ensure that our vision is always open to new ideas: KESSEL – Leading in drainage.

**Photo sheet:**

## ***EasyClean free UnderSink:* a miracle of space**

(Source: KESSEL AG)

Ein Bild, das drinnen, Fräse enthält.

Automatisch generierte Beschreibung

Subtitle: The KESSEL *EasyClean free UnderSink* grease separator is optimised for free-standing set-ups, where space is limited and only small volumes of wastewater are produced.



Subtitle: Manufactured from permanently resistant polymer (PP). That makes it 100 % corrosion-free and resistant to wastewater containing aggressive ingredients such as fatty acids. The material ensures the separator tank is durable, waterproof and odour-tight.



Subtitle: A cover with all-round seal and clip closures simplifies cleaning and maintenance measures. To aid installation and removal, the *EasyClean free UnderSink* grease separator has a quick-release, 360° rotatable and vertically adjustable swivel connection to the pipe.